{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":1,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":17,"n_cols":8,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
[null,"Measurements of unloaded motor speed at 12V and various 50 kHz PWM duty cycle"]
[]
[]
[null,null,null,"Duty Cycle","Motor","Encoder","Pump","Flow"]
[null,null,"Count","%","(rpm)","(Hz)","(rpm)","(ml/min)"]
[null,null,1,0,0,0,0,0]
[null,null,4,0.10344827586206896,0,0,0,0]
[null,null,5,0.13793103448275862,105,56,21,13.125]
[null,null,7,0.20689655172413793,300,160,60,37.5]
[null,null,10,0.3103448275862069,543.75,290,108.75,67.96875]
[null,null,13,0.41379310344827586,781.875,417,156.375,97.734375]
[null,null,16,0.5172413793103449,1042.5,556,208.5,130.3125]
[null,null,21,0.6896551724137931,1398.75,746,279.75,174.84375]
[null,null,24,0.7931034482758621,1674.375,893,334.875,209.296875]
[null,null,27,0.896551724137931,1974.375,1053,394.875,246.796875]
[null,null,30,1,2328.75,1242,465.75,291.09375]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}